## Clutch

#### Clutch Master Cylinder Overhaul

12-6

Exploded View

NOTE:

- RHD type is shown, LHD type is similar.
- When attaching the reservoir hose, align the yellow mark on the hose to the rib on reservoir connection area.
- When attaching the reservoir hose, align the blue mark on the hose to the rib on clutch master cylinder connection area.

1. Clip catches should be on the arrow marked side
2. CONNECTOR
3. O-RING

   Replace

4. O-RING

   Replace

5. CLUTCH LINE CONNECTOR
6. RESERVOIR HOSE

   Inspect for damage, leaks, interference and twisting

7. Clip catches should be on the arrow marked side
8. RESERVOIR
9. RETAINING CLIP

   Replace

10. PISTON ASSEMBLY

    Check for scoring and wear.

11. (Brake Assembly Lube)
12. PUSH ROD
13. CIRCLIP
14. LOCK PIN

    Replace

15. YOKE
16. PEDAL PIN
17. STOPPER

    Check for damage and bending.

18. CLUTCH MASTER CYLINDER SEAL
19. MASTER CYLINDER BODY

    Check the cylinder wall for scoring and wear.

a a a