## Manual Transmission

#### Mainshaft Bearing and Oil Seal Replacement

13-39

Special Tools Required

- Adjustable bearing puller, 25 - 40 mm, 07736-A01000B
- Driver, 07749-0010000
- Attachment, 37 x 40 mm 07746-0010200
- Attachment, 52 x 55 mm 07746-0010400

1. Remove the differential assembly.
2. Remove the ball bearing (A) from the clutch housing (B) using the special tool.

1. 3/8" -16

   SLIDE HAMMER

   (commercially available)

1. Remove the oil seal (A) from the clutch side.

4. Drive the new oil seal in from the transmission side using the special tools.

5. Drive the new ball bearing (A) in from the transmission side using the special tools.