## Engine Lubrication

#### Oil Pump Overhaul (cont'd)

8-13

Oil Pressure Switch Replacement

1. Install the oil pump chain tensioner.

1. Remove the set clip from the oil pump chain tensioner.

1. Install the oil pan (see page 7-28).

1. Disconnect the oil pressure switch connector, then remove the oil pressure switch.

1. Apply liquid gasket to the oil pressure switch threads, then install the oil pressure switch.

a a a