## EPS Components

#### Steering Gearbox Installation (cont'd)

17-24

1. Install the motor on the steering gearbox (see page 17-7).

1. Install the steering joint (A) and reconnect the steering shaft (B) and pinion shaft (C). Make sure the steering joint is connected as follows:

- Insert the upper end of the steering joint onto the steering shaft (line up the bolt hole (D) with the flat portion (E) on the shaft).
- Slip the lower end of the steering joint onto the pinion shaft (line up the bolt hole (F) with the groove (G) around the shaft) and loosely install the lower joint bolt. Be sure that the lower joint bolt is securely in the groove in the pinion shaft.
- Pull on the steering joint to make sure that the steering joint is fully seated. Then install the upper joint bolt and tighten it.

1. Install the driver's dashboard lower covers.

1. Centre the cable reel by first rotating it clockwise until it stops. Then rotate it counterclockwise (about 2 and a half turns) until the arrow mark on the label points straight up. Reinstall the steering wheel.

1. Install the front wheels.

1. After installation, perform the following checks.

- Perform the front toe inspection.
- Check the steering wheel spoke angle. Adjust by turning the right and left tie-rods equally, if necessary.

a a a