## Engine Assembly

#### Engine Removal (cont'd)

5-7

19. Remove the alternator lower bracket (A), then remove the A/C compressor (B) without disconnecting the A/C hose.

20. Remove the radiator cap.
21. Raise the hoist to full height.
22. Remove the front tyres/wheels.
23. Remove the splash shield.

24. Loosen the drain plug in the radiator, drain the engine coolant, refer to the '01 Civic Shop Manual on this CD (see page 10-8).
25. Drain the transmission fluid:

- Manual transmission, refer to the '01 Civic Shop Manual on this CD (see page 13-3).
- Automatic transmission, refer to the '01 Civic Shop Manual on this CD (see page 14-122).

26. Drain the engine oil (see page 8-3).
27. Disconnect the primary heated oxygen sensor (primary HO2S) connector (A) and the secondary heated oxygen sensor (secondary HO2S) connector (B) (Except D16V3 engine).

28. Remove exhaust pipe A (C).