## Engine Assembly

#### Engine Installation (cont'd)

5-12

1. Push the ECM connectors through the bulkhead, then install the grommet (A).

1. Install the harness clamps (B).

1. Install the splash shield.

1. Lower the hoist.

1. Connect the engine control module (ECM) connectors (A) and main wire harness connector (B), then install the ground cable (C).

1. Connect the accelerator pedal sensor connector (A), then install the harness clamp (B).

a a a