## Standards and Service Limits

#### Automatic Transmission and Differential (cont'd)

2-15

Item | Measurement | Qualification | Standard or New
Wire Diameter | O.D. | Free Length | No. of Coil
Secondary valve body springs, refer to the '01 Civic Shop Manual on this CD (see page 14-187) | 3-4 shift valve spring |  | 0.9 mm (0.035 in.) | 7.6 mm (0.299 in.) | 57.0 mm (2.244 in.) | 26.8
2-3 shift valve spring |  | 0.9 mm (0.035 in.) | 7.6 mm (0.299 in.) | 57.0 mm (2.244 in.) | 26.8
4th exhaust valve spring |  | 0.9 mm (0.035 in.) | 6.1 mm (0.240 in.) | 36.4 mm (1.433 in.) | 19.5
3-4 orifice control valve spring |  | 0.7 mm (0.028 in.) | 6.6 mm (0.260 in.) | 37.5 mm (1.476 in.) | 24.6
Servo body springs (see page 14-94) | 1st accumulator spring |  | 2.1 mm (0.083 in.) | 16.0 mm (0.630 in.) | 89.1 mm (3.508 in.) | 16.2
4th accumulator spring A |  | 2.6 mm (0.102 in.) | 17.0 mm (0.669 in.) | 88.4 mm (3.480 in.) | 14.2
4th accumulator spring B |  | 2.3 mm (0.091 in.) | 10.2 mm (0.402 in.) | 51.6 mm (2.031 in.) | 13.8
3rd accumulator spring A |  | 2.8 mm (0.110 in.) | 17.5 mm (0.689 in.) | 94.3 mm (3.713 in.) | 15.6
3rd accumulator spring B |  | 2.1 mm (0.083 in.) | 31.0 mm (1.220 in.) | 38.2 mm (1.504 in.) | 2.4
2nd accumulator spring C |  | 2.2 mm (0.087 in.) | 14.5 mm (0.571 in.) | 68.0 mm (2.677 in.) | 13.9
2nd accumulator spring A |  | 2.4 mm (0.094 in.) | 29.0 mm (1.142 in.) | 39.0 mm (1.535 in.) | 2.9
Lock-up valve body springs, refer to the Civic Shop Manual on this CD (see page 14-189) | Lock-up shift valve spring |  | 0.9 mm (0.035 in.) | 7.6 mm (0.299 in.) | 73.7 mm (2.902 in.) | 32.0
Lock-up timing valve spring |  | 0.9 mm (0.035 in.) | 8.1 mm (0.319 in.) | 80.7 mm (3.177 in.) | 54.2

Item | Measurement | Qualification | Standard or New | Service Limit
A/T differential carrier | Pinion shaft contact area I.D. |  | 18-010-18.028 mm (0.709-0.710 in.) | -
Carrier-to-pinion shaft clearance |  | 0.023-0.057 mm (0.001-0.002 in.) | 0.1 mm (0.004 in.)
Driveshaft contact area I.D. |  | 26.025-26.045 mm (1.0246-1.0254 in.) | -
Carrier-to-driveshaft clearance |  | 0.045-0.086 mm (0.002-0.003 in.) | 0.12 mm (0.005 in.)
Set ring-to-carrier bearing outer race clearance |  | 0-0.15 mm (0-0.006 in.) | Adjust
A/T differential pinion gear | Backlash |  | 0.05-0.15 mm (0.002-0.006 in.) | -
I.D. |  | 18.042-18.066 mm (0.7103-0.7113 in.) | -
Pinion gear-to-pinion shaft clearance |  | 0.055-0.095 mm (0.0022-0.0037 in.) | 0.15 mm (0.006 in.)