## Engine Block

#### Crankshaft Installation (cont'd)

7-27

1. Put the lower block on the cylinder block.

1. Tighten the bearing cap bolts in sequence to 29 Nm (3.0 kgf/m, 22 lbf/ft).

1. Tighten the bearing cap bolts an additional 56`°`.

1. Tighten the 8 mm bolts in sequence to 22 Nm (2.2 kgf/m, 16 lbf/ft).

1. Use the special tools to drive a new oil seal squarely into the block to the specified installed height.

1. Measure the distance between the crankshaft (A) and oil seal (B).

   Oil Seal Installed Height:

5.5 - 6.5 mm (0.22 - 0.26 in.)

a a a