## Clutch

#### Slave Cylinder Overhaul

12-10

NOTE:

- Do not spill brake fluid on the vehicle; it may damage the paint; if brake fluid does contact the paint, wash it off immediately with water.
- Clean all parts in brake fluid and air dry; blow out all passages with compressed air.
- Before reassembling, check that all parts are free of dust and other foreign particles.
- Replace parts with new ones whenever specified to do so.
- Make sure no dirt or other foreign matter is allowed to contaminate the brake fluid.
- Do not mix different brands of brake fluid as they may not be compatible.
- Do not reuse the drained fluid. Use only clean DOT 3 or 4 brake fluid.

1. O-RING

   Replace.

2. BLEEDER SCREW CAP
3. BLEEDER SCREW

   8 Nm (0.8 kgf/m, 5.8 lbf/ft)

4. (Brake Assembly Lube)
5. PISTON CUP

   Replace.

6. SLAVE CYLINDER PISTON

   Check for wear and damage.

7. PUSH ROD
8. Urea Grease UM264

   (P/N 41211-PY5-305)

9. (Brake Assembly Lube)
10. BOOT

    Check that it is fitted securely over the cylinder body.

11. SLAVE CYLINDER SPRING

    Install with small and facing piston.

12. SLAVE CYLINDER BODY

    Check the cylinder wall for scoring and wear

13. CONNECTOR

a a a