## Seats

#### Rear Seat Removal/Installation

20-237

NOTE: Take care not to scratch the body or tear the seat covers.

Remove the rear seat as shown.

Install the seat in the reverse order of removal and note these items:

- Before installing the centre anchor bolts on the seat-back with the centre shoulder belt, make sure there are no twists or kinks in the belt.
- Make sure the seat-backs lock securely.

  Fastener Locations
  A : Bolt, 2 | B : Bolt, 1
  1. PIVOT BUSHING
  2. CENTRE BELT

     (For some models)

  3. RIGHT SEAT-BACK
  4. HINGE COVER
  5. SEAT-BACK CENTRE HINGE
  6. BUSHING
  7. LEFT SEAT BACK
  8. PIVOT BUSHING
  9. LEFT SEAT CUSHION
  10. RIGHT SEAT CUSHION
  11. BUSHING
  12. SEAT BELT BUCKLE
  13. CENTRE ANCHOR BOLT

      7/16-20 UNF, 32 Nm (3.3 kgf m, 24 lbf ft)