## Forward Clutch

#### Clutch Reassembly (cont'd)

14-373

17. If the clearance is out of the service limit, select a new clutch end plate from following table, then recheck.

NOTE: If the thickest clutch end plate is installed, but the clearance is still over the standard, replace the clutch discs and clutch plates.

FORWARD CLUTCH END PLATE

Mark | Part Number | Thickness
15 | 22561-P4V-003 | 3.5 mm (0.138 in.)
16 | 22562-P4V-003 | 3.6 mm (0.142 in.)
17 | 22563-P4V-003 | 3.7 mm (0.146 in.)
18 | 22564-P4V-003 | 3.8 mm (0.150 in.)
19 | 22565-P4V-003 | 3.9 mm (0.154 in.)
20 | 22566-P4V-003 | 4.0 mm (0.157 in.)
21 | 22567-P4V-003 | 4.1 mm (0.161 in.)
22 | 22568-P4V-003 | 4.2 mm (0.165 in.)
23 | 22569-P4V-003 | 4.3 mm (0.169 in.)
24 | 22570-P4V-003 | 4.4 mm (0.173 in.)
25 | 22571-P4V-003 | 4.5 mm (0.177 in.)
26 | 22572-P4V-003 | 4.6 mm (0.181 in.)
27 | 22573-P4V-003 | 4.7 mm (0.185 in.)
14 | 22574-P4V-003 | 3.4 mm (0.134 in.)

18. After replacing the clutch end plate, make sure that the clearance is within tolerance.