## SRS

#### DTC Troubleshooting Index

23-40

NEC (M2), DENSO (M1) SRS unit (Without Side Airbag Model)

DTC | Detection Item | Notes
1-1 | Open in driver's airbag inflator | (see page 23-55)
1-2 | Increased resistance in driver's airbag inflator | (see page 23-55)
1-3 | Short to another wire or decreased resistance in driver's airbag inflator | (see page 23-57)
1-4 | Short to power in driver's airbag inflator | (see page 23-59)
1-5 | Short to ground in driver's airbag inflator | (see page 23-61)
2-1 | Open in front passenger's airbag inflator | (see page 23-63)
2-2 | Increased resistance in front passenger's airbag inflator | (see page 23-63)
2-3 | Short to another wire or decreased resistance in front passenger's airbag inflator | (see page 23-64)
2-4 | Short to power in front passenger's airbag inflator | (see page 23-66)
2-5 | Short to ground in front passenger's airbag inflator | (see page 23-67)
3-1 | Open in left side seat belt tensioner | (see page 23-69)
3-2 | Increased resistance in left side seat belt tensioner | (see page 23-69)
3-3 | Short to another wire or decreased resistance in left side seat belt tensioner | (see page 23-71)
3-4 | Short to power in left side seat belt tensioner | (see page 23-73)
3-5 | Short to ground in left side seat belt tensioner | (see page 23-75)
4-1 | Open in right side seat belt tensioner | (see page 23-77)
4-2 | Increased resistance in right side seat belt tensioner | (see page 23-77)
4-3 | Short to another wire or decreased resistance in left side seat belt tensioner | (see page 23-79)
4-4 | Short to power in left side seat belt tensioner | (see page 23-81)
4-5 | Short to ground in left side seat belt tensioner | (see page 23-83)