## Seats

#### Front Seat Cover Replacement (cont'd)

20-93

8. With side airbag: Remove the side airbag (see page 23-169, and release the hooks (A) from the airbag module holder (B).

9. Release the hooks (A) and hook springs (B), then loosen the seat-back cover (C).

10. Pull out the headrest guides (A) while pinching the end of the guides, and remove them.

11. Pull back the seat-back cover all the way around, then remove it.
12. Install the cover in the reverse order of removal, and note these items:

- To prevent wrinkles when installing a seat-back cover, make sure the material is stretched evenly over the pad before securing the hooks and hook springs.
- Make sure the side airbag harness and OPDS harness (passenger's seat) are routed properly.
- If necessary, reinstall the OPDS control unit (see page 23-39).