## Clutch

#### Slave Cylinder Overhaul

12-10

NOTE:

- Do not spill brake fluid on the vehicle; it may damage the paint; if brake fluid does contact the paint, wash it off immediately with water.
- Clean all parts in brake fluid and air dry; blow out all passages with compressed air.
- Before reassembling, check that all parts are free of dust and other foreign particles.
- Replace parts with new ones whenever specified to do so.
- Make sure no dirt or other foreign matter is allowed to contaminate the brake fluid.
- Do not mix different brands of brake fluid as they may not be compatible.
- Do not reuse the drained fluid. Use only clean DOT 3 brake fluid.

  1. (Brake Assembly Lube)
  2. SLAVE CYLINDER SPRING

     Install with small end facing piston.

  3. SLAVE CYLINDER BODY

     Check the cylinder wall for scoring and wear.

  4. O-RING

     Replace.

  5. BLEEDER SCREW CAP
  6. BLEEDER SCREW

     8 Nm (0.8 kgf/m, 5.8 lbf/ft)

  7. BOOT

     Check that it is fitted securely over the cylinder body.

  8. (Brake Assembly Lube)
  9. Urea Grease UM264

     (P/N 41211-PY5 -305)

  10. PUSH ROD
  11. SLAVE CYLINDER PISTON

      Check for wear and damage.

  12. PISTON CUP

      Replace.