## EPS Components

#### Steering Gearbox Overhaul

17-13

Exploded View

1. MOTOR CONNECTOR
2. MOTOR
3. O-RINGS

   Replace.

4. PINION SHAFT GROMMET
5. TORQUE SENSOR
6. GEARBOX HOUSING
7. SPRING
8. RACK GUIDE SCREW
9. LOCKNUT
10. RACK HOUSING
11. STOP RING

    Replace.

12. LOCK SCREW

    162 Nm (16.5 kgf/m, 119 lbf/ft)

    Replace.

13. SLIDER GUIDE
14. BOOT BAND

    Replace.

15. TIE-ROD END
16. TIE-ROD

    54 Nm (5.5 kgf/m, 40 lbf/ft)

17. LOCK WASHER

    Replace.

18. BRACKET
19. O-RINGS

    Replace.

20. STOP PLATE

    Replace.

21. BOOT
22. BOOT BAND

    Replace.

23. DISC WASHER
24. RACK GUIDE

a a a