## Transmission Range Switch

#### Transmission Range Switch Installation

14-385

1. Set the control lever (A) to position by turning it.

NOTE: Do not squeeze the end of the control shaft tips (B) together when turning into position. If the tips are squeezed together it will cause a faulty signal or position due to the play between the control shaft and the switch.

2. Align the cutouts (A) on the rotary-frame with the neutral positioning cutouts (B) on the transmission range switch, then put a 2.0 mm (0.08 in.) feeler gauge blade (C) in the cutouts to hold it in the position.

   NOTE: Be sure to use a 2.0 mm (0.08 in.) blade or equivalent to hold the switch in the position.

3. Install the transmission range switch (A) gently on the control shaft (B) with holding the position with the 2.0 mm (0.08 in.) blade (C).

4. Tighten the bolts on the transmission range switch while you continue to hold the position.

   Do not move the transmission range switch when tightening the bolts. Remove the feeler gauge.