## Glass

#### Rear Window Replacement (cont'd)

20-26

11. Glue the clips (A) and fasteners (B) to the inside face of the rear window (C) as shown:

- Be sure the clips and fasteners line up with the alignment marks (D).
- Be careful not to touch the rear window where adhesive will be applied.

12. Install the clips (A) to the rear window opening flange (B) and glue the fasteners (C) to the offset area of the rear shelf (D).

Fastener Locations

A : Clip, 2B : Fastener, 2

13. Set the rear window in the opening and centre it. Make alignment marks (A) across the rear window and body with a grease pencil at the 4 points shown. Be careful not to touch the rear window where adhesive will be applied.

14. Remove the rear window.