## Design Specifications

#### (cont'd)

2-29

Item | Measurement | Qualification | Specification
WHEEL ALIGNMENT | Camber | Front | 0°
Rear | -0°45'
Caster | Front | 1°33'
Total toe | Front | 0 mm (0 in.)
Rear | In 2 mm (1/16 in.)
BRAKE | Type of service brake | Front | Power-assisted self-adjusting ventilated disc
Rear | Power-assisted self-adjusting solid disc or drum
Type of parking brake |  | Mechanical actuating, rear wheels
Pad friction surface area | Front | 35 cm2 x 2 (5.4 sq in. x 2)
Shoe friction surface area | Rear | 67 cm2 x 2 (10.3 sq in. x 2)
TYRES | Size of front and rear tyre (4-door) | KE (1.4S), KG (1.4S, 1.6 LS), KB, KQ (GLI), KH (EXI), KN (150I), KU (EXI), KY, KF, KV, KT models | 184/70R14 88H
KK, KX models | 185/70R14 86H M + S
KM, KP models | 185/65R15 88H
KE (1.6SE), KG (1.6LS, 1.6ES) KQ (VTI), KH (VTI), KN (170I) KU (VTI, VTI-S) models | 195/60R15 88H
Size of front and rear tyre (5-door) | KE (1.4S, 1.4LS), KT models | 185/70R 14 88H
KE (1.6S, 1.6LS, 1.6ES), KQ models | 195/60R 15 88H
Size of spare tyre | KQ, KN, KU, KX models | T125/70D15 95M
AIR CONDITIONING | Cooling capacity |  | 3,870 kcal/h (15,400 BTU/h)
Compressor | Type/manufacturer | Scroll/SANDEN
Number of cylinders | -
Capacity | 85.7 ml/rev. (5.23 cu in./rev.)
Maximum speed | 12,000 rpm
Lubricant capacity | 130 ml (4 1/3 fl oz)
Lubricant type | SP-10 (P/N 38897-P13-A01AH or 38899-P13-A01)
Condenser | Type | Corrugated fin
Evaporator | Type | Corrugated fin
Blower | Type | Radial fan
Motor type | 190 W/12 V
Speed control | 9-speed
Maximum capacity | 480 m3/h (16,900 cu ft/h)
Temperature clutch |  | Air-mix type
Compressor clutch | Type | Dry, single plate, poly-V belt drive
Electrical power consumption at 20°C (68°F) | 42 W maximum at 12 V
Refrigerant | Type | HFC-134a (R-134a)
Quantity | 500-550 g (17.5-19.5 oz)