## Engine Block

#### Flywheel Removal and Installation

7-5
Drive Plate Removal and Installation

Special Tools Required Ring Gear Holder, 07LAB-PV00100 Remove the six flywheel bolts, then separate the flywheel from the crankshaft flange. After installation, tighten the bolts in a criss-cross pattern.

1. Inspect ring gear teeth for wear or damage.

Remove the six drive plate bolts, then separate the drive plate from the crankshaft flange. After installation, tighten the bolts in a criss-cross pattern.