## SRS

#### General Troubleshooting Information (cont'd)

23-34

Reading the SRS Indicator Light Method (with service check connector (2P) models): The SRS indicator light indicates the DTC by the number of blinks when the SCS short connector is connected to the service check connector (2P).

1. Make sure the ignition switch is OFF and wait for 10 seconds. Then connect the SCS short connector (A) to the service check connector (2P) (B). If you do not wait 10 seconds, the SRS unit will not be completely reset or output DTCs.

4-door

1. SRS INDICATOR LIGHT

5-door

1. SRS INDICATOR LIGHT

2. Turn the ignition switch ON (II). The SRS indicator light comes on for about 6 seconds and then goes off. Then it will indicate the DTC.

3. Read the DTC.
4. Turn the ignition switch OFF and wait for 10 seconds. Then disconnect the SCS short connector from the service check connector (2P).