## Cylinder Head

#### Crankshaft Pulley Removal and Installation (cont'd)

6-17

Installation

1. Remove any oil from the pulleys (A), guide plate (B), crankshaft (C), bolt (D) and washer (E). Clean and lubricate as shown below.

O: Clean

X: Remove any oil

: Lubricate

2. Install the crankshaft pulley and hold the pulley with holder handle (A) and holder attachment (B).

With P/S:

With EPS:

3. Tighten the bolt to 20 Nm (2.0 kgf/m, 14 lbf/ft) with a torque wrench and 19 mm socket (C). Do not use an impact wrench.
4. Tighten the pulley bolt an additional 90o.