## Relays

#### Power Relay Test

22-8

Use this chart to identify the type of relay, then do the test listed for it.

Relay | Test
SHIFT LOCK RELAY | 5 terminal type
KEY INTERLOCK RELAY (KG model: daytime running lights)

5-terminal type

Check for continuity between the terminals.

- There should be continuity between the No. 1 and No. 2 terminals when power and ground are connected to the No. 3 and No. 5 terminals.
- There should be no continuity between the No. 1 and No. 4 terminals when power is disconnected.