## Manual Transmission

#### Transmission Installation (cont'd)

13-14

1. Remove the chain hoist and engine hanger from the engine.

1. Install the air cleaner housing mounting bracket bolt (A), water pipe mounting bolts (B), harness cover (C).

1. Apply Urea Grease UM264 (P/N 41211-PY5-305) to the end of the slave cylinder rod. Install the slave cylinder. Take care not to bend the clutch line.

1. Install the harness clip.

1. Install the cable bracket (A) and cables (B).

a a a