## Interior Trim

#### Carpet Replacement (cont'd)

20-71

3. RHD: Detach the clips, then remove the footrest (A).

   Fastener Locations
   : Clip, 2

4. Using a utility knife, cut the carpet (A) under the heater area (B) on the driver's side, and cut out the shift lever area (C) and parking brake lever area (D) as shown. Release the hook (E), then pull back the carpet.

5. Remove the clip (A), and release the fasteners (B), then remove the carpet (C).

   Fastener Location
   A: Clip, 1