## Seat Heaters

#### Seat Heater Switch Test/Replacement

22-207

4-door:

1. Remove the centre console switch panel (see page 20-73).
2. Disconnect the 10P connector (A) from the seat heater switch (B), then remove the switch.

3. Check for continuity in each switch position according to the table.

5-door:

1. Remove the parking brake cover (see step 3 on page 20-213).
2. Disconnect the 6P connector (A) from the seat heater switch (B), then remove the switch.

3. Check for continuity in each switch position according to the table.