## Conventional Brake Components

#### Front Brake Calliper Overhaul (cont'd)

19-17

KX Model

: Use recommended rubber grease in the calliper seal set.

: Use recommended seal grease in the calliper seal set.

1. CALLIPER PIN A
2. BOOTS
3. BANJO BOLT

   3.4 Nm (3.5 kgf/m, 25 lbf/ft)

4. BRAKE HOSE
5. BLEED SCREW

   9 Nm (0.9 kgf/m, 7 lbf/ft)

6. CALLIPER BODY
7. PISTON SEAL

   replace.

8. BOOT CLIP

   Replace.

9. PISTON BOOT

   Replace.

10. PISTON
11. BRAKE PADS
12. SEALING WASHERS

    Replace.

13. PAD RETAINERS
14. OUTER PAD SHIM
15. WEAR INDICATOR

    Install inner pad with its wear indicator downward

16. CALLIPER BRACKET
17. PISTON BOOT

    Replace.

18. CALLIPER PIN B
19. BUSHING