## Transmission Housing

#### Housing and Shaft Assemblies Removal (cont'd)

14-176

Special Tools Required Housing puller, 07HAC-PK40102 NOTE: Refer to the Exploded View as needed during the following procedure.

1. Remove the mainshaft speed sensor and sensor washer.
   NOTE: The mainshaft speed sensor washer is equipped on the SLXA transmission; the BMXA transmission does not have the washer.
2. Remove the transmission housing mounting bolts, transmission hanger and connector bracket.
3. Align the spring pin (A) on the control shaft (B) with the transmission housing groove (C) by turning the control shaft.
   NOTE: Be careful not to squeeze the end of the control shaft tips together when turning the shaft. If the tips are squeezed together it will cause a faulty signal or position due to the play between the control shaft and the switch.

4. Install the special tool over the mainshaft, then remove the transmission housing.
   NOTE: If the top arm of your housing puller is too short, replace it with Housing Puller Arm, 205 mm, 07SAC-P0Z0101.

5. Remove the countershaft reverse gear collar, countershaft reverse gear and needle bearing.

6. Remove the lock bolt securing the shift fork, then remove the shift fork with the reverse selector together.
7. Remove the mainshaft sub-assembly (A) and countershaft sub-assembly (B) together.

8. Remove the differential assembly.