## Glass

#### Rear Window Replacement (cont'd)

20-27

15. With a sponge, apply a light coat of glass primer along the edge of the rear window (A) and moulding (B) as shown, then lightly wipe it off with gauze or cheesecloth:

- Do not apply body primer to the rear window and do not get body and glass primer sponges mixed up.
- Never touch the primed surfaces with your hands. If you do, the adhesive may not bond to the rear window properly, causing a leak after the rear window is installed.
- Keep water, dust and abrasive materials away from the primed surface.

Cross-hatched area: Apply glass primer here

16. With a sponge, apply a light coat of body primer to the original adhesive remaining around the rear window opening flange. Let the body primer dry for at least 10 minutes:

- Do not apply glass primer to the body and be careful not to mix up glass and body primer sponges.
- Never touch the primed surfaces with your hands.

Cross-hatched area: Apply body primer here

17. Before filling a cartridge, cut a ''V'' in the end of the nozzle (A) as shown.