## Mirrors

#### Carpet Replacement

20-6

LHD SRS components are located in this area. Review the SRS component locations (see page 23-24) and the precautions and procedures (see page 23-25) in the SRS section before performing repairs or service. Refer to the '01 Civic Shop Manual, P/N 62S5A00 on this CD.

NOTE:

- Put on gloves to protect your hands.
- Take care not to damage, wrinkle or twist the carpet.
- Be careful not to damage the dashboard or other interior trim pieces.

1. Remove these items, refer to the '01 Civic Shop Manual, P/N 62S5A00 on this CD:

- Front seats, both sides (see page 20-229)
- Rear seat cushion, both sides (see page 20-237)
- Kick panels, both sides (see page 20-206)
- Front door sill trim, both sides (see page 20-206)
- Rear door sill trim, both sides (see page 20-206)
- Dashboard centre lower cover (see page 20-217)
- Driver's dashboard under cover (see page 20-216)
- Passenger's dashboard lower cover (see page 20-220)
- Parking brake cover (see step 3 on page 20-213)

2. Remove the nut (A) and using a hex wrench, release the clip (B), then remove the footrest (C).

Fastener Locations

A : Nut, 1B : Clip, 1

3. Using a utility knife, cut the carpet (A) under the heater area (B) on the driver's side, then pull back the carpet.

4. Remove the clips (A) and release the fasteners (B), then remove the carpet (C).

Fastener Locations

A : Clip, 3

5. Remove the rear floor carpet, refer to the '01 Civic Shop Manual, P/N 62S5A00 on this CD (see step 6 on page 20-214)