## Rear Floor

#### Removal

3-33

- Cut the rear floor 15 mm (0.6 in.) from the welded flange of the rear cross-member.
- If necessary, replace the rear frame B.
- Check the rear floor cross-member position for damage.
- If necessary, replace the rear floor cross-member.

  1. REAR FLOOR CROSS-MEMBER
  2. REAR FLOOR
  3. Cut line
  4. REAR FLOOR CROSS-MEMBER
  5. REAR FLOOR
  6. REAR FLOOR CROSS-MEMBER
  7. REAR FRAME A
  8. VIEW (Z)
  9. REAR FRAME B
  10. REAR FRAME A
  11. REAR FRAME B