## Power Mirrors

#### Power Mirror Actuator Replacement (cont'd)

22-151

7. Remove the three screws and the actuator (A).

8. Remove the three mounting screws and separate the actuator (A) from the actuator bracket (B).

9. Route the wire harness (A) of the new actuator through the hole in the bracket (B).

10. Insert the new actuator terminals into the connector in the original arrangement as shown below.

    Left | Right

Wire side of female terminals

*1: With defogger

*2: With retract mirror

11. Reassemble the mirror in the reverse order of disassembly.
    Be careful not to break in the mirror holder when installing it to the actuator.
12. After installing, check the power mirror operation.