## Forward Clutch

#### Clutch Reassembly

14-369

Special Tools Required

- Clutch spring compressor set, 07LAE-PX40000
  - Clutch spring compressor attachment, 07LAE-PX40100
  - Clutch spring compressor attachment, 07HAE-PL50101
  - Clutch spring compressor bolt assembly, 07GAE-PG40200

- Snap ring pliers, 07LGC-0010100

1. Inspect the check valve (A); if it's loose, replace the piston (B).

2. Install new O-rings (A) on the piston (B).

3. Install the piston (A) in the clutch drum (B). Apply pressure and rotate to ensure proper seating.

   Lubricate the piston O-ring with ATF before installing. Do not pinch the O-ring by installing the piston with too much force.