## Seat Belts

#### Front Seat Belt Replacement (cont'd)

23-17

Seat Belt Buckle

1. If equipped with a side airbag, disconnect the negative battery cable and wait at least 3 minutes before beginning work.
2. Remove the front seat (see page 20-229).
3. Remove the centre cover from the seat, driver's seat (see page 20-231), passenger's seat (see page 20-232).
4. Detach the seat belt switch connector clip (A) and harness clip (B).

Driver's seat:

Passenger's seat:

5. On the driver's seat, adjust the seat cushion to its maximum height.

6. Remove the centre anchor bolt (A) and remove the seat belt buckle (B).

7. Pull the seat belt switch harness (C) out through the space between the seat cushion and the seat linkage (driver's seat), or the hole on the seat track (passenger's seat).
8. Install the buckle in the reverse order of removal and note these items:

- Assemble the washers on the centre anchor bolt as shown.
- If equipped with a side airbag, reconnect the negative cable to the battery.

1. CENTRE ANCHOR BOLT
2. TOOTHED LOCK WASHER
3. SPRING WASHER
4. COLLAR
5. CENTRE ANCHOR