## Wiper/Washers

#### Wiper/Washer Switch Test/Replacement (cont'd)

22-171

5. Inspect the connector terminals to be sure they are all making good contact.

- If the terminals are bent, loose or corroded, repair them as necessary, and recheck the system.
- If the terminals look OK, check for continuity between the terminals in each switch position according to the tables.

- If there is no continuity, replace the switch.

Windshield:

Rear Window (5 - door):

[ ] : RHD type except KE