## Wipers/Washers

#### Washer Motor Test

22-13

Headlight Washer Nozzle Replacement

1. Remove the left inner fender, refer to the '01 Civic Shop Manual on this CD (see page 20-121).
2. Disconnect each 2P connector from the washer motor.

3. Test the motor by connecting battery power to the No.1 terminal and ground the No.2 terminal of the washer motor. The motor should run.

- If the motor does not run or fails to run smoothly, replace it.
- If the motor runs smoothly, but little or no washer fluid is pumped, check for a disconnected or blocked washer hose, or a clogged pump outlet in the motor.

1. Remove the front bumper, refer to the '01 Civic Shop Manual on this CD (see page 20-104).
2. Disconnect the tube (A) from the washer nozzle (B).

3. Pull the washer nozzle lid (A) out and remove it from the nozzle (B).

4. Remove the two screws and the washer nozzle.
5. Install in the reverse order of removal.

a a a