## Engine Assembly

#### Engine Installation (cont'd)

5-19

32. Install the EVAP canister hose.

33. Install the shift cable (A) and shift cable (B) using the plastic washer (C), washer (D) and new cotter pins (E) (M/T).

34. Install the clutch slave cylinder (A) and clutch line bracket mounting bolt (B) (M/T).

35. Install the Battery base.
36. Install the intake air duct (A) and ground cable (B).