## Valve Body

#### Valve Bodies and ATF Strainer Removal

14-179

Exploded View

1. LOCK-UP SEPARATOR PLATE
2. LOCK-UP VALVE BODY
3. 6 x 1.0 mm, 7 Bolts
4. ATF FEED PIPE

   (7-position)

5. DOWEL PIN
6. 6 X 1.0 mm, 1 Bolt
7. DOWEL PIN
8. O-RING

   Replace.

9. DETENT ARM SHAFT
10. WASHER
11. DETENT ARM
12. CONTROL SHAFT
13. ATF FEED PIPE

    8 x 62 mm

14. ATF FEED PIPE

    8 x 40 mm

15. ATF FEED PIPE

    8 x 145 mm

16. 6 x 1.0 mm, 1 Bolt
17. ATF STRAINER
18. 6 x 1.0 mm, 8 Bolts
19. SERVO BODY
20. SERVO SEPARATOR PLATE
21. 6 x 1.0 mm, 3 Bolts
22. SECONDARY VALVE BODY
23. STOP SHAFT BRACKET
24. DOWEL PIN, 8 x 40 mm
25. SECONDARY SEPARATOR PLATE
26. ATF FEED PIPE,

    8 x 118 mm

27. ATF PUMP DRIVE GEAR
28. TORQUE CONVERTER HOUSING
29. DOWEL PIN
30. MAIN SEPARATOR PLATE
31. ATF PUMP DRIVEN GEAR
32. ATF PUMP DRIVEN GEAR SHAFT
33. MAIN VALVE BODY
34. 6 x 1.0 mm, 5 Bolts
35. ATF FEED PIPE, 8 x 112 mm
36. STATOR SHAFT STOP
37. STATOR SHAFT
38. ATF FEED PIPE, 8 x 138.8 mm
39. TORQUE CONVERTER CHECK VALVE
40. TORQUE CONVERTER CHECK VALVE SPRING
41. COOLER RELIEF
42. COOLER RELIEF VALVE SPRING
43. ATF FEED PIPE,

    8 x 220 mm, (7-position)

44. REGULATOR VALVE BODY