## Sunroof

#### Sunshade Replacement (cont'd)

20-198

Motor Replacement

6. Release both rear sunshade base sliders (A) from the guide rail portions of the frame, then remove the sunshade.

7. Remove both front sunshade base sliders (A).

8. Install the sunshade in the reverse order of removal, and check the glass height adjustment (see page 20-194).
9. Check for water leaks. Let the water run freely from a hose without a nozzle. Do not use a high-pressure spray.

1. Remove the headliner (see page 20-210).

2. Put on gloves to protect your hands. Disconnect the connector (A) and remove the bolts, then remove the motor (B).

   Fastener Locations
   : Bolt, 2

3. Install the motor in the reverse order of removal and note these items:

- Make sure the connector is plugged in properly.
- Check the motor operation.