## Manual Transmission

#### Countershaft Reassembly

13-34

Exploded View

1. Turkey-produced D14Z6 engine transmission
2. *1: DOUBLE CONE SYNCHRO TYPE

   *2: SINGLE CONE SYNCHRO TYPE

3. LOCKNUT

   Replace.

   127 to 0 to 127 Nm

   13 to 0 to 13 kgf/m,

   94 to 0 to 94 lbf/ft

4. SPRING WASHER
5. BALL BEARING

   Check for wear and operation.

6. NEEDLE BEARING

   Check for wear and operation.

7. 5TH GEAR
8. 4TH GEAR
9. 3RD GEAR
10. 2ND GEAR
11. NEEDLE BEARING

    Check for wear and operation.

12. SPACER
13. FRICTION DAMPER

    Check for wear and damage.

14. SYNCHRO RING
15. SYNCHRO SPRING
16. REVERSE GEAR
17. 1ST/2ND SYNCHRO HUB
18. UP
19. DOUBLE CONE SYNCHRO
20. COUNTERSHAFT
21. NEEDLE BEARING

    Check for wear and operation.

22. 1ST GEAR
23. FRICTION DAMPER

    Check for wear and damage.

24. SYNCHRO RING
25. SYNCHRO SPRING