## Cylinder Head

#### Cam Chain Removal (cont'd)

6-15

1. Loosely install the crankshaft pulley.

1. Turn the crankshaft counterclockwise to compress the auto-tensioner.

1. Align the holes on the lock (A) and the auto-tensioner (B), then insert a 1.5 mm (0.06 in.) diameter pin (C) into the holes. Turn the crankshaft clockwise to secure the pin.

1. Remove the auto-tensioner.

1. Remove the cam chain guide B.

a a a