## SRS

#### DTC Troubleshooting (cont'd)

23-93

14. Turn the ignition switch OFF.

15. Connect the special tool (Jumper) to the FSR1i connector (A).

16. Check resistance between the No. 1 and No. 12 terminals of the U1o connector. There should be 1 ohm or less.

U1o CONNECTOR

Wire side of female terminals

Is the resistance as specified?

YES - Faulty right front sensor or SRS unit. Replace the right front sensor; if the problem is still present, replace the SRS unit.

NO - Faulty engine compartment wire harness or dashboard wire harness B; replace the faulty harness.