## Honda Multi Matic Transmission/CVT Differential

#### Carrier Bearing Side Clearance Inspection

14-390

Special Tools Required Driver 40 mm I.D., 07746-0030100

1. Install the 80 mm set ring (A) in the transmission housing (B).

2. Install the differential assembly (A) in the transmission housing (B) using the special tool.

3. Install the three dowel pins (A) and the gasket (B) on the transmission housing (C).

4. Place the flywheel housing (D) on the transmission housing.
5. Install the housing bolts (20 bolts) and tighten the bolts in two or more steps to 29 Nm (3.0 kgf/m, 22 lbf/ft) in a criss-cross pattern.