## Plastic Parts Paint

#### Use of the Repair Material (reference)

6-13

NOTE: Follow the materials manufacturer's instructions. The use of a special polyester putty for PP bumper is described here:

1. Filler

   Mixing Ratio:

2. Sanding filler
   Spray bumper primer (see page 6-19) on the area where the PP material was used.
3. Primer surfacer
   The primer surfacer is used to protect the PP resin surface and fill cavities or flaws before the intermediate coat and top coat.

Use the 2-component type primer surfacer (grey).

Mixing Ratio:

4. Intermediate coat and top coat

Use the 2-part polyester urethane top coat. Top coat is also used for an intermediate coat.

Mixing Ratio:

NOTE: Be sure to mix the correct amount of the hardener and softener.

NOTE: Use a spray gun to apply the paint. Do not use a brush.

Drying time:

Air dry 20°C (68°F) | 6~10 minutes Touch dry
Almost hardened | 12~24 hours
Thoroughly hardened | 96 hours

Force dry the intermediate coat and top coat.

NOTE: Mix only an amount that can be used before it hardens.