## Seats

#### Rear Seat Removal/Installation – Fixed Type

20-96

NOTE: Take care not to scratch the body or tear the seat covers.

Remove the rear seat as shown.

Install the seat in the reverse order of removal, and note these items:

- Before attaching the rear seat-back and cushion, make sure there are no twists or kinks in the rear seat belts and centre belt.
- When installing the seat cushion, slip the seat belt buckles through the slits in the seat cushion.

  Fastener Locations
  A : Bolt, 1 | B : Bolt, 2 or 3
  1. With armrest only
  2. HOOKS
  3. SEAT-BACK
  4. HOOK
  5. COLLAR
  6. HOOK
  7. CLIP
  8. SEAT CUSHION
  9. REAR SEAT BELT BUCKLE
  10. CENTRE BELT
  11. CLIP
  12. HOOK
  13. REAR SEAT BELT BUCKLE
  14. CENTRE BELT BUCKLE
  15. SLITS