## Standards and Service Limits

#### Automatic Transmission and Differential (cont'd)

2-13

Item | Measurement | Qualification | Standard or New | Service Limit
Reverse idler gear | Reverse idler gear shaft diameter at needle bearing contact area |  | 13.990-14.000 mm (0.5508-0.5512 in.) | When worn or damaged
I.D. |  | 18.007-18.020 mm (0.7089-0.7094 in.) | When worn or damaged
End play |  | 0.05-0.18 mm (0.002-0.007 in.) | -
I.D. of reverse idler gear shaft holder |  | 14.416-14.434 mm (0.5676-0.5683 in.) | When worn or damaged
Sub-shaft | Diameter of needle bearing contact area | at transmission housing | 25.991-26.000 mm (1.023-1.024 in.) | When worn or damaged
at 4th gear collar | 23.9935-23.0065 mm (0.9446-0.9058 in.) | When worn or damaged
4th gear I.D. |  | 32.000-32.016 mm (1.2600-1.2605 in.) | When worn or damaged
4th gear end play |  | 0.05-0.17 mm (0.002-0.007 in.) | -
4th gear collar length |  | 24.0-24.1 mm (0.945-0.949 in.) | -
4th gear collar flange thickness |  | 2.95-3.10 mm (0.116-0.122 in.) | When worn or damaged
4th gear thrust washer thickness |  | 2.93-3.00 mm (0.115-0.118 in.) | When worn or damaged
1st-clutch feed pipe O.D. | at 15 mm (0.6 in.) from end | 7.97-7.98 mm (0.3138-0.3142 in.) | 7.95 mm (0.313 in.)

Item | Measurement | Qualification | Standard or New
|  |  | Wire Diameter | O.D. | Free Length | No. of Coil
Main valve body springs (see page 14-183) | Relief valve spring |  | 1.1 mm (0.043 in.) | 8.6 mm (0.339 in.) | 37.1 mm (1.4161 in.) | 13.4
Modulator valve spring |  | 1.4 mm (0.055 in) | 9.4 mm (0.370 in.) | 33.8 mm (1.331 in.) | 10.9
CPB valve spring |  | 1.0 mm (0.039 in.) | 8.1 mm (0.319 in.) | 40.9 mm (1.610 in.) | 16.2
1-2 shift valve spring |  | 0.9 mm (0.035 in.) | 7.6 mm (0.299 in.) | 41.3 mm (1.626 in.) | 16.3
2nd orifice control valve spring |  | 0.7 mm (0.028 in.) | 6.6 mm (0.260 in.) | 34.8 mm (1.370 in.) | 22.0
Servo control valve spring |  | 1.0 mm (0.039 in.) | 8.1 mm (0.319 in.) | 52.1 mm (2.051 in.) | 20.8
Regulator valve body springs (see page 14-186) | Stator reaction spring |  | 4.5 mm (0.177 in.) | 35.4 mm (1.394 in.) | 30.3 mm (1.193 in.) | 1.9
Regulator valve spring A |  | 1.9 mm (0.075 in.) | 14.7 mm (0.579 in.) | 77.4 mm (3.047 in.) | 15.2
Regulator valve spring B |  | 1.8 mm (0.071 in.) | 9.6 mm (0.378 in.) | 44.0 mm (1.732 in.) | 12.6
Cooler relief valve spring |  | 1.0 mm (0.039 in.) | 8.4 mm (0.331 in.) | 33.8 mm (1.331 in.) | 8.2
Torque converter check valve spring |  | 1.0 mm (0.039 in.) | 8.4 mm (0.331 in.) | 33.8 mm (1.331 in.) | 8.2
Lock-up control valve spring |  | 0.8 mm (0.031 in.) | 6.0 mm (0.236 in.) | 38.4 mm (1.512 in.) | 30.3