## Power Windows

#### Master Switch Test

22-8

1. Remove the power window master switch. (see page 22-9).
2. Disconnect the 14P connector from the switch (A).

3. Check for continuity between the terminals in each switch position according to the table.

Driver's Switch:

The driver's switch is combined with the control unit so you cannot isolate the switch to test it. Instead, run the master switch input test procedures on page 22-6. If the tests are normal, the driver's switch must be faulty.

Passenger's Switch:

[ ]: RHD type

4. If the switch is faulty, replace the switch.

a a a