## Honda Multi Matic Transmission/CVT Differential

#### Differential Carrier/Final Driven Gear Replacement

14-388

Carrier Bearing Replacement

1. Remove the final driven gear from the differential carrier. The final driven gear bolts have left-hand threads.

2. Install the final driven gear with the chamfered side on the inner bore (A) facing the differential carrier.
3. Tighten the bolts to 98 Nm (10.0 kgf/m, 72 lbf/ft) in a criss-cross pattern.

Special Tools Required

Driver 40 mm I.D., 07746-0030100

1. Remove the bearings (A) with a commercially available bearing puller (B) and stepper adapter (C).

2. Install the new bearings with the special tool and a press. Press the bearing on until it bottoms.