## Power Mirrors

#### Power Mirror Actuator Replacement

22-149

4-door:

1. Remove the mirror holder the power mirror (see page 20-33).
2. Remove the power mirror (see page 20-33) and disconnect the connector.
3. Remove the cover (A) and two screws from the mirror connector (B).

4. Record the terminal locations and wire colours.
5. Cut the wire harness with the wire cutter.

6. Remove the three mounting screws and separate the mirror housing (A) from the bracket (B).

7. Remove the three mounting screws and separate the actuator bracket (A) from the mirror housing (B).

8. Remove the three mounting screws and separate the actuator (A) from the actuator bracket (B).