## Glass

#### Quarter Glass Replacement (cont'd)

20-190

14. With a sponge, apply a light coat of body primer to the original adhesive remaining around the quarter glass opening flange. Let the body primer dry for at least 10 minutes:

- Do not apply glass primer to the body and be careful not to mix up glass and body primer sponges.
- Never touch the primed surfaces with your hands.

Hatched area: Apply body primer here.

15. Before filling a cartridge, cut a ''V'' in the end of the nozzle (A) as shown.

16. Pack adhesive into the cartridge without air pockets to ensure continuous delivery. Put the cartridge in a caulking gun and run a bead of adhesive (A) around the edge of the glass (B) as shown. With the alignment lines (C) on the quarter glass as a guide, apply the adhesive to the upper and lower corner portions of the quarter glass. Apply the adhesive within 30 minutes after applying the glass primer. Make a slightly thicker bead at each corner.