## Manual Transmission

#### Transmission Disassembly (cont'd)

13-17

1 2 3 4 5

6

7

8

9

TRANSMISSION HOUSING

10 mm WASHER

Replace.

10 mm FLANGE BOLT

44 Nm (4.5 kgf/m, 33 lbf/ft)

8 mm FLANGE BOLT

27 Nm (2.8 kgf/m, 20 lbf/ft)

TRANSMISSION HANGER A

INTERLOCK BOLT

39 Nm (4.0 kgf/m, 29 lbf/ft)

OIL GUIDE PLATE M

72 mm SHIM

OIL GUTTER PLATE

10

11

12

13

14

15

16

17

18

19

80 mm SHIM

8 x 14 mm DOWEL PIN

CHANGE LEVER ASSEMBLY

6 mm FLANGE BOLT

12 Nm (1.2 kgf/m, 9 lbf/ft)

DETENT BOLT

22 Nm (2.2 kgf/m, 16 lbf/ft)

12 mm WASHER

Replace.

SPRING

STEEL BALL

CLUTCH LINE CLIP BRACKET

HARNESS STAY

20

21

22

23

24

25

26

TRANSMISSION HANGER B

20 mm WASHER

Replace.

FILLER PLUG

44 Nm (4.5 kgf/m, 33 lbf/ft)

40 x 56 x 8 mm OIL SEAL

Replace.

14 mm WASHER

Replace.

DRAIN PLUG

39 Nm (4.0 kgf/m, 29 lbf/ft)

32 mm SEALING CAP

34 Nm (3.5 kgf/m, 25 lbf/ft)

a a a